# Static Call Graph - [MR16\MR16.axf]

# Static Call Graph for image MR16\MR16.axf

#<CALLGRAPH># ARM Linker, 5060960: Last Updated: Sun Nov 30 10:55:27 2025

### Maximum Stack Usage = 344 bytes + Unknown(Cycles, Untraceable Function Pointers)

### Call chain for Maximum Stack Depth:

main ⇒ LCD_DrawString ⇒ LCD_DrawChar ⇒ LCD_DrawPoint ⇒ LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout

### Mutually Recursive functions

- ADC1_2_IRQHandler ⇒ ADC1_2_IRQHandler
- BusFault_Handler ⇒ BusFault_Handler
- HardFault_Handler ⇒ HardFault_Handler
- MemManage_Handler ⇒ MemManage_Handler
- NMI_Handler ⇒ NMI_Handler
- UART_EndRxTransfer ⇒ UART_EndRxTransfer
- UART_EndTxTransfer ⇒ UART_EndTxTransfer
- UsageFault_Handler ⇒ UsageFault_Handler

  ### Function Pointers

  - ADC1_2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - BusFault_Handler from stm32f1xx_it.o(i.BusFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_RX1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - CAN1_SCE_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel2_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel2_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel3_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel3_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel5_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel5_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel6_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel6_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - DMA1_Channel7_IRQHandler from stm32f1xx_it.o(i.DMA1_Channel7_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - DebugMon_Handler from stm32f1xx_it.o(i.DebugMon_Handler) referenced from startup_stm32f103xb.o(RESET)
  - EXTI0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI15_10_IRQHandler from stm32f1xx_it.o(i.EXTI15_10_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - EXTI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - EXTI9_5_IRQHandler from stm32f1xx_it.o(i.EXTI9_5_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - FLASH_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - HardFault_Handler from stm32f1xx_it.o(i.HardFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C1_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_ER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - I2C2_EV_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - MemManage_Handler from stm32f1xx_it.o(i.MemManage_Handler) referenced from startup_stm32f103xb.o(RESET)
  - NMI_Handler from stm32f1xx_it.o(i.NMI_Handler) referenced from startup_stm32f103xb.o(RESET)
  - OnRxDone from sx1281.o(i.OnRxDone) referenced from sx1281.o(.data)
  - OnRxError from sx1281.o(i.OnRxError) referenced from sx1281.o(.data)
  - OnRxTimeout from sx1281.o(i.OnRxTimeout) referenced from sx1281.o(.data)
  - OnTxDone from sx1281.o(i.OnTxDone) referenced from sx1281.o(.data)
  - OnTxTimeout from sx1281.o(i.OnTxTimeout) referenced from sx1281.o(.data)
  - PVD_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - PendSV_Handler from stm32f1xx_it.o(i.PendSV_Handler) referenced from startup_stm32f103xb.o(RESET)
  - RCC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_Alarm_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - RTC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - Reset_Handler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - SPI_DMAError from stm32f1xx_hal_spi.o(i.SPI_DMAError) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)
  - SPI_DMAError from stm32f1xx_hal_spi.o(i.SPI_DMAError) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)
  - SPI_DMAHalfReceiveCplt from stm32f1xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)
  - SPI_DMAHalfTransmitCplt from stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)
  - SPI_DMAHalfTransmitReceiveCplt from stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)
  - SPI_DMAReceiveCplt from stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)
  - SPI_DMATransmitCplt from stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)
  - SPI_DMATransmitReceiveCplt from stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt) referenced from stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)
  - SVC_Handler from stm32f1xx_it.o(i.SVC_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SX1281Calibrate from sx1281_driver.o(i.SX1281Calibrate) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281ClearIrqStatus from sx1281_driver.o(i.SX1281ClearIrqStatus) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetFirmwareVersion from sx1281_driver.o(i.SX1281GetFirmwareVersion) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetFrequencyError from sx1281_driver.o(i.SX1281GetFrequencyError) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetIrqStatus from sx1281_driver.o(i.SX1281GetIrqStatus) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetOpMode from sx1281_driver.o(i.SX1281GetOpMode) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetPacketStatus from sx1281_driver.o(i.SX1281GetPacketStatus) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetPacketType from sx1281_driver.o(i.SX1281GetPacketType) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetPayload from sx1281_driver.o(i.SX1281GetPayload) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetRssiInst from sx1281_driver.o(i.SX1281GetRssiInst) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetRxBufferStatus from sx1281_driver.o(i.SX1281GetRxBufferStatus) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281GetStatus from sx1281_driver.o(i.SX1281GetStatus) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalGetDioStatus from sx1281_driver_hal.o(i.SX1281HalGetDioStatus) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalReadBuffer from sx1281_driver_hal.o(i.SX1281HalReadBuffer) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalReadCommand from sx1281_driver_hal.o(i.SX1281HalReadCommand) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalReadRegister from sx1281_driver_hal.o(i.SX1281HalReadRegister) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalReadRegisters from sx1281_driver_hal.o(i.SX1281HalReadRegisters) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalReset from sx1281_driver_hal.o(i.SX1281HalReset) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalWriteBuffer from sx1281_driver_hal.o(i.SX1281HalWriteBuffer) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalWriteCommand from sx1281_driver_hal.o(i.SX1281HalWriteCommand) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalWriteRegister from sx1281_driver_hal.o(i.SX1281HalWriteRegister) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281HalWriteRegisters from sx1281_driver_hal.o(i.SX1281HalWriteRegisters) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281Init from sx1281_driver.o(i.SX1281Init) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281OnDioIrq from sx1281_driver.o(i.SX1281OnDioIrq) referenced from sx1281_driver.o(.data)
  - SX1281SendPayload from sx1281_driver.o(i.SX1281SendPayload) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetAutoFS from sx1281_driver.o(i.SX1281SetAutoFS) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetAutoTx from sx1281_driver.o(i.SX1281SetAutoTx) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetBleAccessAddress from sx1281_driver.o(i.SX1281SetBleAccessAddress) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetBleAdvertizerAccessAddress from sx1281_driver.o(i.SX1281SetBleAdvertizerAccessAddress) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetBufferBaseAddresses from sx1281_driver.o(i.SX1281SetBufferBaseAddresses) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetCad from sx1281_driver.o(i.SX1281SetCad) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetCadParams from sx1281_driver.o(i.SX1281SetCadParams) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetCrcPolynomial from sx1281_driver.o(i.SX1281SetCrcPolynomial) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetCrcSeed from sx1281_driver.o(i.SX1281SetCrcSeed) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetDioIrqParams from sx1281_driver.o(i.SX1281SetDioIrqParams) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetFs from sx1281_driver.o(i.SX1281SetFs) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetInterruptMode from sx1281_driver.o(i.SX1281SetInterruptMode) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetLongPreamble from sx1281_driver.o(i.SX1281SetLongPreamble) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetModulationParams from sx1281_driver.o(i.SX1281SetModulationParams) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetPacketParams from sx1281_driver.o(i.SX1281SetPacketParams) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetPacketType from sx1281_driver.o(i.SX1281SetPacketType) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetPayload from sx1281_driver.o(i.SX1281SetPayload) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetPollingMode from sx1281_driver.o(i.SX1281SetPollingMode) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetRegistersDefault from sx1281_driver.o(i.SX1281SetRegistersDefault) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetRegulatorMode from sx1281_driver.o(i.SX1281SetRegulatorMode) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetRfFrequency from sx1281_driver.o(i.SX1281SetRfFrequency) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetRx from sx1281_driver.o(i.SX1281SetRx) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetRxDutyCycle from sx1281_driver.o(i.SX1281SetRxDutyCycle) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetSaveContext from sx1281_driver.o(i.SX1281SetSaveContext) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetSleep from sx1281_driver.o(i.SX1281SetSleep) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetStandby from sx1281_driver.o(i.SX1281SetStandby) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetSyncWord from sx1281_driver.o(i.SX1281SetSyncWord) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetSyncWordErrorTolerance from sx1281_driver.o(i.SX1281SetSyncWordErrorTolerance) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetTx from sx1281_driver.o(i.SX1281SetTx) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetTxContinuousPreamble from sx1281_driver.o(i.SX1281SetTxContinuousPreamble) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetTxContinuousWave from sx1281_driver.o(i.SX1281SetTxContinuousWave) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetTxParams from sx1281_driver.o(i.SX1281SetTxParams) referenced from sx1281_driver_hal.o(.constdata)
  - SX1281SetWhiteningSeed from sx1281_driver.o(i.SX1281SetWhiteningSeed) referenced from sx1281_driver_hal.o(.constdata)
  - SysTick_Handler from stm32f1xx_it.o(i.SysTick_Handler) referenced from startup_stm32f103xb.o(RESET)
  - SystemInit from system_stm32f1xx.o(i.SystemInit) referenced from startup_stm32f103xb.o(.text)
  - TAMPER_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_BRK_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_CC_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_TRG_COM_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM1_UP_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM2_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - TIM4_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UART_DMAAbortOnError from stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError) referenced from stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)
  - UART_DMAError from stm32f1xx_hal_uart.o(i.UART_DMAError) referenced from stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA)
  - UART_DMAReceiveCplt from stm32f1xx_hal_uart.o(i.UART_DMAReceiveCplt) referenced from stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA)
  - UART_DMARxHalfCplt from stm32f1xx_hal_uart.o(i.UART_DMARxHalfCplt) referenced from stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA)
  - USART1_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USART2_IRQHandler from stm32f1xx_it.o(i.USART2_IRQHandler) referenced from startup_stm32f103xb.o(RESET)
  - USART3_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USBWakeUp_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_HP_CAN1_TX_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - USB_LP_CAN1_RX0_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - UsageFault_Handler from stm32f1xx_it.o(i.UsageFault_Handler) referenced from startup_stm32f103xb.o(RESET)
  - WWDG_IRQHandler from startup_stm32f103xb.o(.text) referenced from startup_stm32f103xb.o(RESET)
  - __main from entry.o(.ARM.Collect$$$$00000000) referenced from startup_stm32f103xb.o(.text)
  - fputc from sx1281_header.o(i.fputc) referenced from printfa.o(i.__0printf)
  - main from main.o(i.main) referenced from entry9a.o(.ARM.Collect$$$$0000000B)
  - tx_cplt_cb from sx1281_driver_spi.o(i.tx_cplt_cb) referenced from sx1281_driver_spi.o(i.SpiInit)
  - txrx_cplt_cb from sx1281_driver_spi.o(i.txrx_cplt_cb) referenced from sx1281_driver_spi.o(i.SpiInit)

  ### Global Symbols

  __main (Thumb, 0 bytes, Stack size unknown bytes, entry.o(.ARM.Collect$$$$00000000))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  _main_stk (Thumb, 0 bytes, Stack size unknown bytes, entry2.o(.ARM.Collect$$$$00000001))

  _main_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Calls]

  - >> __scatterload

  __main_after_scatterload (Thumb, 0 bytes, Stack size unknown bytes, entry5.o(.ARM.Collect$$$$00000004))
  [Called By]

  - >> __scatterload

  _main_clock (Thumb, 0 bytes, Stack size unknown bytes, entry7b.o(.ARM.Collect$$$$00000008))

  _main_cpp_init (Thumb, 0 bytes, Stack size unknown bytes, entry8b.o(.ARM.Collect$$$$0000000A))

  _main_init (Thumb, 0 bytes, Stack size unknown bytes, entry9a.o(.ARM.Collect$$$$0000000B))

  __rt_lib_shutdown_fini (Thumb, 0 bytes, Stack size unknown bytes, entry12b.o(.ARM.Collect$$$$0000000E))

  __rt_final_cpp (Thumb, 0 bytes, Stack size unknown bytes, entry10a.o(.ARM.Collect$$$$0000000F))

  __rt_final_exit (Thumb, 0 bytes, Stack size unknown bytes, entry11a.o(.ARM.Collect$$$$00000011))

  Reset_Handler (Thumb, 8 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  ADC1_2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Calls]

  - >> ADC1_2_IRQHandler
  [Called By]
  - >> ADC1_2_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  CAN1_RX1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  CAN1_SCE_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  DMA1_Channel4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  FLASH_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C1_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_ER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  I2C2_EV_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  PVD_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RCC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_Alarm_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  RTC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SPI2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TAMPER_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_BRK_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_CC_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_TRG_COM_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM1_UP_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM2_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  TIM4_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART1_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USART3_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USBWakeUp_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_HP_CAN1_TX_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  USB_LP_CAN1_RX0_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  WWDG_IRQHandler (Thumb, 0 bytes, Stack size 0 bytes, startup_stm32f103xb.o(.text))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  __aeabi_llsr (Thumb, 32 bytes, Stack size 0 bytes, llushr.o(.text))
  [Called By]

  - >> __aeabi_d2uiz
  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_d2ulz

  _ll_ushift_r (Thumb, 0 bytes, Stack size 0 bytes, llushr.o(.text), UNUSED)

  __aeabi_memcpy (Thumb, 36 bytes, Stack size 0 bytes, memcpya.o(.text))
  [Called By]

  - >> SX1281HalReadRegisters
  - >> SX1281HalWriteRegisters
  - >> SX1281HalWriteCommand
  - >> SX1281HalWriteBuffer
  - >> SX1281HalReadCommand
  - >> SX1281HalReadBuffer

  __aeabi_memcpy4 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memcpy8 (Thumb, 0 bytes, Stack size 0 bytes, memcpya.o(.text), UNUSED)

  __aeabi_memset (Thumb, 14 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Called By]

  - >> _memset$wrapper
  - >> __aeabi_memclr

  __aeabi_memset4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memset8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  __aeabi_memclr (Thumb, 4 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  __aeabi_memclr4 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text))
  [Called By]

  - >> USAR_UART_IDLECallback
  - >> MX_TIM1_Init
  - >> SystemClock_Config

  __aeabi_memclr8 (Thumb, 0 bytes, Stack size 0 bytes, memseta.o(.text), UNUSED)

  _memset$wrapper (Thumb, 18 bytes, Stack size 8 bytes, memseta.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_memset

  strcpy (Thumb, 18 bytes, Stack size 0 bytes, strcpy.o(.text))
  [Called By]

  - >> USAR_UART_IDLECallback

  __aeabi_dmul (Thumb, 228 bytes, Stack size 48 bytes, dmul.o(.text))
  [Stack]

  - Max Depth = 88
  - Call Chain = __aeabi_dmul ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> SX1281GetFrequencyError
  - >> _fp_digits

  __aeabi_ddiv (Thumb, 222 bytes, Stack size 32 bytes, ddiv.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = __aeabi_ddiv ⇒ _double_round
  [Calls]
  - >> _double_round
  [Called By]
  - >> SX1281SetRfFrequency
  - >> SX1281GetFrequencyError
  - >> _fp_digits

  __aeabi_i2d (Thumb, 34 bytes, Stack size 16 bytes, dflti.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_i2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> SX1281GetFrequencyError

  __aeabi_ui2d (Thumb, 26 bytes, Stack size 16 bytes, dfltui.o(.text))
  [Stack]

  - Max Depth = 56
  - Call Chain = __aeabi_ui2d ⇒ _double_epilogue ⇒ _double_round
  [Calls]
  - >> _double_epilogue
  [Called By]
  - >> SX1281SetRfFrequency

  __aeabi_d2uiz (Thumb, 50 bytes, Stack size 8 bytes, dfixui.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = __aeabi_d2uiz
  [Calls]
  - >> __aeabi_llsr
  [Called By]
  - >> SX1281SetRfFrequency

  __aeabi_uidiv (Thumb, 0 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)

  __aeabi_uidivmod (Thumb, 44 bytes, Stack size 12 bytes, uidiv.o(.text), UNUSED)
  [Called By]

  - >> _printf_core

  __aeabi_uldivmod (Thumb, 98 bytes, Stack size 40 bytes, uldiv.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _printf_core
  - >> _fp_digits

  __I$use$fp (Thumb, 0 bytes, Stack size 8 bytes, iusefp.o(.text), UNUSED)

  _double_round (Thumb, 30 bytes, Stack size 8 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 8
  - Call Chain = _double_round
  [Called By]
  - >> __aeabi_ddiv
  - >> _double_epilogue
  - >> __aeabi_dadd

  _double_epilogue (Thumb, 156 bytes, Stack size 32 bytes, depilogue.o(.text))
  [Stack]

  - Max Depth = 40
  - Call Chain = _double_epilogue ⇒ _double_round
  [Calls]
  - >> __aeabi_llsr
  - >> __aeabi_llsl
  - >> _double_round
  [Called By]
  - >> __aeabi_ui2d
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_dadd

  __aeabi_dadd (Thumb, 322 bytes, Stack size 48 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_lasr
  - >> __aeabi_llsl
  - >> _double_round
  - >> _double_epilogue
  [Called By]
  - >> __aeabi_drsub
  - >> __aeabi_dsub
  - >> _fp_digits

  __aeabi_dsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_drsub (Thumb, 6 bytes, Stack size 0 bytes, dadd.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_dadd

  __aeabi_d2ulz (Thumb, 48 bytes, Stack size 0 bytes, dfixul.o(.text), UNUSED)
  [Calls]

  - >> __aeabi_llsr
  - >> __aeabi_llsl
  [Called By]
  - >> _fp_digits

  __aeabi_cdrcmple (Thumb, 48 bytes, Stack size 0 bytes, cdrcmple.o(.text), UNUSED)
  [Called By]

  - >> _fp_digits

  __scatterload (Thumb, 28 bytes, Stack size 0 bytes, init.o(.text))
  [Calls]

  - >> __main_after_scatterload
  [Called By]
  - >> _main_scatterload

  __scatterload_rt2 (Thumb, 0 bytes, Stack size 0 bytes, init.o(.text), UNUSED)

  __aeabi_llsl (Thumb, 30 bytes, Stack size 0 bytes, llshl.o(.text))
  [Called By]

  - >> __aeabi_uldivmod
  - >> _double_epilogue
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz

  _ll_shift_l (Thumb, 0 bytes, Stack size 0 bytes, llshl.o(.text), UNUSED)

  __aeabi_lasr (Thumb, 36 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)
  [Called By]

  - >> __aeabi_dadd

  _ll_sshift_r (Thumb, 0 bytes, Stack size 0 bytes, llsshr.o(.text), UNUSED)

  BSP_SPI_GetHandle (Thumb, 18 bytes, Stack size 0 bytes, spi_1.o(i.BSP_SPI_GetHandle))
  [Called By]

  - >> BSP_SPI_TransmitReceive
  - >> BSP_SPI_Transmit
  - >> BSP_SPI_GetState

  BSP_SPI_GetState (Thumb, 24 bytes, Stack size 8 bytes, spi_1.o(i.BSP_SPI_GetState))
  [Stack]

  - Max Depth = 8
  - Call Chain = BSP_SPI_GetState
  [Calls]
  - >> HAL_SPI_GetState
  - >> BSP_SPI_GetHandle
  [Called By]
  - >> LCD_WriteDataBuffer_DMA

  BSP_SPI_RegisterCallback (Thumb, 22 bytes, Stack size 0 bytes, spi_1.o(i.BSP_SPI_RegisterCallback))
  [Called By]

  - >> SpiInit

  BSP_SPI_Transmit (Thumb, 42 bytes, Stack size 8 bytes, spi_1.o(i.BSP_SPI_Transmit))
  [Stack]

  - Max Depth = 104
  - Call Chain = BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_SPI_Transmit_DMA
  - >> HAL_SPI_Transmit
  - >> BSP_SPI_GetHandle
  [Called By]
  - >> SpiIn
  - >> LCD_WriteDataBuffer_DMA
  - >> LCD_WriteDataBuffer
  - >> LCD_WriteData
  - >> LCD_WriteCommand

  BSP_SPI_TransmitReceive (Thumb, 46 bytes, Stack size 16 bytes, spi_1.o(i.BSP_SPI_TransmitReceive))
  [Stack]

  - Max Depth = 128
  - Call Chain = BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_SPI_TransmitReceive_DMA
  - >> HAL_SPI_TransmitReceive
  - >> BSP_SPI_GetHandle
  [Called By]
  - >> SpiInOut

  BSP_UART_GetHandle (Thumb, 10 bytes, Stack size 0 bytes, uart.o(i.BSP_UART_GetHandle))
  [Called By]

  - >> fputc

  BusFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.BusFault_Handler))
  [Calls]

  - >> BusFault_Handler
  [Called By]
  - >> BusFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DMA1_Channel2_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel2_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel2_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DMA1_Channel3_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel3_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel3_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DMA1_Channel5_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel5_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel5_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DMA1_Channel6_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel6_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel6_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DMA1_Channel7_IRQHandler (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DMA1_Channel7_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = DMA1_Channel7_IRQHandler ⇒ HAL_DMA_IRQHandler
  [Calls]
  - >> HAL_DMA_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  DebugMon_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.DebugMon_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  EXTI15_10_IRQHandler (Thumb, 8 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.EXTI15_10_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = EXTI15_10_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler ⇒ HAL_GPIO_EXTI_Callback
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  EXTI9_5_IRQHandler (Thumb, 24 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.EXTI9_5_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = EXTI9_5_IRQHandler ⇒ HAL_GPIO_EXTI_IRQHandler ⇒ HAL_GPIO_EXTI_Callback
  [Calls]
  - >> HAL_GPIO_EXTI_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  Error_Handler (Thumb, 4 bytes, Stack size 0 bytes, main.o(i.Error_Handler))
  [Called By]

  - >> HAL_UART_MspInit
  - >> HAL_SPI_MspInit
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  - >> MX_TIM1_Init
  - >> MX_SPI2_Init
  - >> MX_SPI1_Init

  GpioGetBitPos (Thumb, 48 bytes, Stack size 0 bytes, sx1281_driver_gpio.o(i.GpioGetBitPos))
  [Called By]

  - >> MSP_GetIRQn
  - >> GpioSetIrq

  GpioInit (Thumb, 2 bytes, Stack size 0 bytes, sx1281_driver_gpio.o(i.GpioInit))
  [Called By]

  - >> SX1281_BSPInit

  GpioRead (Thumb, 4 bytes, Stack size 0 bytes, sx1281_driver_gpio.o(i.GpioRead))
  [Calls]

  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> SX1281HalGetDioStatus

  GpioSetIrq (Thumb, 50 bytes, Stack size 16 bytes, sx1281_driver_gpio.o(i.GpioSetIrq))
  [Stack]

  - Max Depth = 32
  - Call Chain = GpioSetIrq ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> MSP_GetIRQn
  - >> GpioGetBitPos
  [Called By]
  - >> SX1281HalIoIrqInit

  GpioWrite (Thumb, 6 bytes, Stack size 0 bytes, sx1281_driver_gpio.o(i.GpioWrite))
  [Calls]

  - >> HAL_GPIO_WritePin
  [Called By]
  - >> SX1281HalReset
  - >> SX1281HalReadRegisters
  - >> SX1281HalWriteRegisters
  - >> SX1281HalWriteCommand
  - >> SX1281HalWriteBuffer
  - >> SX1281HalReadCommand
  - >> SX1281HalReadBuffer

  HAL_DMA_Abort (Thumb, 70 bytes, Stack size 8 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Abort))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> HAL_UART_DMAStop

  HAL_DMA_Abort_IT (Thumb, 148 bytes, Stack size 8 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Abort_IT))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_DMA_Abort_IT
  [Called By]
  - >> HAL_UART_IRQHandler

  HAL_DMA_IRQHandler (Thumb, 316 bytes, Stack size 40 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_DMA_IRQHandler
  [Called By]
  - >> DMA1_Channel7_IRQHandler
  - >> DMA1_Channel6_IRQHandler
  - >> DMA1_Channel5_IRQHandler
  - >> DMA1_Channel3_IRQHandler
  - >> DMA1_Channel2_IRQHandler

  HAL_DMA_Init (Thumb, 84 bytes, Stack size 12 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Init))
  [Stack]

  - Max Depth = 12
  - Call Chain = HAL_DMA_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_SPI_MspInit

  HAL_DMA_Start_IT (Thumb, 112 bytes, Stack size 16 bytes, stm32f1xx_hal_dma.o(i.HAL_DMA_Start_IT))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> DMA_SetConfig
  [Called By]
  - >> HAL_SPI_Transmit_DMA
  - >> HAL_SPI_TransmitReceive_DMA
  - >> UART_Start_Receive_DMA

  HAL_Delay (Thumb, 32 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_Delay))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_Delay
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SX1281_Running
  - >> SX1281_Init
  - >> LCD_Init
  - >> main
  - >> SX1281HalReset

  HAL_GPIO_EXTI_Callback (Thumb, 40 bytes, Stack size 24 bytes, gpio_1.o(i.HAL_GPIO_EXTI_Callback))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_GPIO_EXTI_Callback
  [Called By]
  - >> HAL_GPIO_EXTI_IRQHandler

  HAL_GPIO_EXTI_IRQHandler (Thumb, 18 bytes, Stack size 8 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_EXTI_IRQHandler))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_GPIO_EXTI_IRQHandler ⇒ HAL_GPIO_EXTI_Callback
  [Calls]
  - >> HAL_GPIO_EXTI_Callback
  [Called By]
  - >> EXTI9_5_IRQHandler
  - >> EXTI15_10_IRQHandler

  HAL_GPIO_Init (Thumb, 446 bytes, Stack size 40 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_GPIO_Init
  [Called By]
  - >> HAL_UART_MspInit
  - >> HAL_TIM_MspPostInit
  - >> HAL_SPI_MspInit
  - >> MX_GPIO_Init

  HAL_GPIO_ReadPin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_ReadPin))
  [Called By]

  - >> SX1281HalWaitOnBusy
  - >> GpioRead

  HAL_GPIO_WritePin (Thumb, 10 bytes, Stack size 0 bytes, stm32f1xx_hal_gpio.o(i.HAL_GPIO_WritePin))
  [Called By]

  - >> MX_GPIO_Init
  - >> LCD_Init
  - >> GpioWrite
  - >> LCD_WriteDataBuffer_DMA
  - >> LCD_WriteDataBuffer
  - >> LCD_WriteData
  - >> LCD_WriteCommand

  HAL_GetTick (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_GetTick))
  [Called By]

  - >> SPI_WaitFlagStateUntilTimeout
  - >> SPI_DMATransmitReceiveCplt
  - >> SPI_DMATransmitCplt
  - >> SPI_DMAReceiveCplt
  - >> HAL_UART_Transmit
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> HAL_Delay
  - >> HAL_SPI_TransmitReceive
  - >> HAL_SPI_Transmit
  - >> UART_WaitOnFlagUntilTimeout

  HAL_HalfDuplex_Init (Thumb, 110 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_HalfDuplex_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_HalfDuplex_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> MX_USART1_UART_Init

  HAL_IncTick (Thumb, 12 bytes, Stack size 0 bytes, stm32f1xx_hal.o(i.HAL_IncTick))
  [Called By]

  - >> SysTick_Handler

  HAL_Init (Thumb, 32 bytes, Stack size 8 bytes, stm32f1xx_hal.o(i.HAL_Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_Init ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_MspInit
  - >> HAL_InitTick
  - >> HAL_NVIC_SetPriorityGrouping
  [Called By]
  - >> main

  HAL_InitTick (Thumb, 54 bytes, Stack size 16 bytes, stm32f1xx_hal.o(i.HAL_InitTick))
  [Stack]

  - Max Depth = 32
  - Call Chain = HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config
  [Called By]
  - >> HAL_RCC_ClockConfig
  - >> HAL_Init

  HAL_MspInit (Thumb, 52 bytes, Stack size 8 bytes, stm32f1xx_hal_msp.o(i.HAL_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_MspInit
  [Called By]
  - >> HAL_Init

  HAL_NVIC_EnableIRQ (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_EnableIRQ))
  [Called By]

  - >> HAL_UART_MspInit
  - >> MX_GPIO_Init
  - >> MX_DMA_Init
  - >> GpioSetIrq

  HAL_NVIC_SetPriority (Thumb, 60 bytes, Stack size 16 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriority))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_NVIC_SetPriority
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_UART_MspInit
  - >> MX_GPIO_Init
  - >> MX_DMA_Init
  - >> HAL_InitTick
  - >> GpioSetIrq

  HAL_NVIC_SetPriorityGrouping (Thumb, 26 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.HAL_NVIC_SetPriorityGrouping))
  [Called By]

  - >> HAL_Init

  HAL_RCC_ClockConfig (Thumb, 280 bytes, Stack size 32 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_ClockConfig))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_GetSysClockFreq
  - >> HAL_InitTick
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_RCC_GetPCLK1Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK1Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetPCLK2Freq (Thumb, 20 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetPCLK2Freq))
  [Called By]

  - >> UART_SetConfig

  HAL_RCC_GetSysClockFreq (Thumb, 64 bytes, Stack size 0 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_GetSysClockFreq))
  [Called By]

  - >> HAL_RCC_ClockConfig

  HAL_RCC_OscConfig (Thumb, 778 bytes, Stack size 40 bytes, stm32f1xx_hal_rcc.o(i.HAL_RCC_OscConfig))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_RCC_OscConfig
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SystemClock_Config

  HAL_SPI_ErrorCallback (Thumb, 50 bytes, Stack size 16 bytes, spi_1.o(i.HAL_SPI_ErrorCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_ErrorCallback
  [Calls]
  - >> SPI_Get
  [Called By]
  - >> SPI_DMATransmitReceiveCplt
  - >> SPI_DMATransmitCplt
  - >> SPI_DMAReceiveCplt
  - >> SPI_DMAError

  HAL_SPI_GetState (Thumb, 6 bytes, Stack size 0 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_GetState))
  [Called By]

  - >> BSP_SPI_GetState

  HAL_SPI_Init (Thumb, 178 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_MspInit
  [Called By]
  - >> MX_SPI2_Init
  - >> MX_SPI1_Init

  HAL_SPI_MspInit (Thumb, 284 bytes, Stack size 48 bytes, spi.o(i.HAL_SPI_MspInit))
  [Stack]

  - Max Depth = 88
  - Call Chain = HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_DMA_Init
  - >> HAL_GPIO_Init
  - >> Error_Handler
  [Called By]
  - >> HAL_SPI_Init

  HAL_SPI_RxCpltCallback (Thumb, 50 bytes, Stack size 16 bytes, spi_1.o(i.HAL_SPI_RxCpltCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_RxCpltCallback
  [Calls]
  - >> SPI_Get
  [Called By]
  - >> SPI_DMAReceiveCplt

  HAL_SPI_RxHalfCpltCallback (Thumb, 50 bytes, Stack size 16 bytes, spi_1.o(i.HAL_SPI_RxHalfCpltCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_RxHalfCpltCallback
  [Calls]
  - >> SPI_Get
  [Called By]
  - >> SPI_DMAHalfReceiveCplt

  HAL_SPI_Transmit (Thumb, 358 bytes, Stack size 40 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_EndRxTxTransaction
  - >> HAL_GetTick
  [Called By]
  - >> BSP_SPI_Transmit

  HAL_SPI_TransmitReceive (Thumb, 496 bytes, Stack size 56 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive))
  [Stack]

  - Max Depth = 112
  - Call Chain = HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_EndRxTxTransaction
  - >> HAL_GetTick
  [Called By]
  - >> BSP_SPI_TransmitReceive

  HAL_SPI_TransmitReceive_DMA (Thumb, 252 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_SPI_TransmitReceive_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  [Called By]
  - >> BSP_SPI_TransmitReceive

  HAL_SPI_Transmit_DMA (Thumb, 190 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_SPI_Transmit_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  [Called By]
  - >> BSP_SPI_Transmit

  HAL_SPI_TxCpltCallback (Thumb, 30 bytes, Stack size 8 bytes, spi_1.o(i.HAL_SPI_TxCpltCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SPI_TxCpltCallback
  [Calls]
  - >> SPI_Get
  [Called By]
  - >> SPI_DMATransmitCplt

  HAL_SPI_TxHalfCpltCallback (Thumb, 50 bytes, Stack size 16 bytes, spi_1.o(i.HAL_SPI_TxHalfCpltCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_TxHalfCpltCallback
  [Calls]
  - >> SPI_Get
  [Called By]
  - >> SPI_DMAHalfTransmitCplt

  HAL_SPI_TxRxCpltCallback (Thumb, 50 bytes, Stack size 16 bytes, spi_1.o(i.HAL_SPI_TxRxCpltCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_TxRxCpltCallback
  [Calls]
  - >> SPI_Get
  [Called By]
  - >> SPI_DMATransmitReceiveCplt

  HAL_SPI_TxRxHalfCpltCallback (Thumb, 50 bytes, Stack size 16 bytes, spi_1.o(i.HAL_SPI_TxRxHalfCpltCallback))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_SPI_TxRxHalfCpltCallback
  [Calls]
  - >> SPI_Get
  [Called By]
  - >> SPI_DMAHalfTransmitReceiveCplt

  HAL_SYSTICK_Config (Thumb, 40 bytes, Stack size 8 bytes, stm32f1xx_hal_cortex.o(i.HAL_SYSTICK_Config))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_SYSTICK_Config
  [Calls]
  - >> __NVIC_SetPriority
  [Called By]
  - >> HAL_InitTick

  HAL_TIMEx_ConfigBreakDeadTime (Thumb, 84 bytes, Stack size 8 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_ConfigBreakDeadTime))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIMEx_ConfigBreakDeadTime
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIMEx_MasterConfigSynchronization (Thumb, 92 bytes, Stack size 16 bytes, stm32f1xx_hal_tim_ex.o(i.HAL_TIMEx_MasterConfigSynchronization))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_TIMEx_MasterConfigSynchronization
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_Base_Init (Thumb, 90 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_Base_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_Base_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_Base_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_Base_MspInit (Thumb, 30 bytes, Stack size 8 bytes, tim.o(i.HAL_TIM_Base_MspInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_TIM_Base_MspInit
  [Called By]
  - >> HAL_TIM_Base_Init

  HAL_TIM_ConfigClockSource (Thumb, 220 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_ConfigClockSource))
  [Stack]

  - Max Depth = 24
  - Call Chain = HAL_TIM_ConfigClockSource ⇒ TIM_TI2_ConfigInputStage
  [Calls]
  - >> TIM_TI2_ConfigInputStage
  - >> TIM_TI1_ConfigInputStage
  - >> TIM_ITRx_SetConfig
  - >> TIM_ETR_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_MspPostInit (Thumb, 64 bytes, Stack size 24 bytes, tim.o(i.HAL_TIM_MspPostInit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_GPIO_Init
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_PWM_ConfigChannel (Thumb, 204 bytes, Stack size 16 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_ConfigChannel))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_ConfigChannel ⇒ TIM_OC4_SetConfig
  [Calls]
  - >> TIM_OC4_SetConfig
  - >> TIM_OC3_SetConfig
  - >> TIM_OC1_SetConfig
  - >> TIM_OC2_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_PWM_Init (Thumb, 90 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_Init))
  [Stack]

  - Max Depth = 28
  - Call Chain = HAL_TIM_PWM_Init ⇒ TIM_Base_SetConfig
  [Calls]
  - >> HAL_TIM_PWM_MspInit
  - >> TIM_Base_SetConfig
  [Called By]
  - >> MX_TIM1_Init

  HAL_TIM_PWM_MspInit (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.HAL_TIM_PWM_MspInit))
  [Called By]

  - >> HAL_TIM_PWM_Init

  HAL_UARTEx_RxEventCallback (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UARTEx_RxEventCallback))
  [Called By]

  - >> HAL_UART_IRQHandler
  - >> UART_Receive_IT
  - >> UART_DMARxHalfCplt
  - >> UART_DMAReceiveCplt

  HAL_UART_DMAStop (Thumb, 112 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_DMAStop))
  [Stack]

  - Max Depth = 16
  - Call Chain = HAL_UART_DMAStop ⇒ HAL_DMA_Abort
  [Calls]
  - >> HAL_DMA_Abort
  - >> UART_EndTxTransfer
  - >> UART_EndRxTransfer
  [Called By]
  - >> USAR_UART_IDLECallback

  HAL_UART_ErrorCallback (Thumb, 34 bytes, Stack size 8 bytes, uart.o(i.HAL_UART_ErrorCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UART_ErrorCallback
  [Calls]
  - >> UART_Get
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> UART_DMAError
  - >> UART_DMAAbortOnError

  HAL_UART_IRQHandler (Thumb, 616 bytes, Stack size 24 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler))
  [Stack]

  - Max Depth = 40
  - Call Chain = HAL_UART_IRQHandler ⇒ UART_Receive_IT ⇒ HAL_UART_RxCpltCallback
  [Calls]
  - >> HAL_DMA_Abort_IT
  - >> HAL_DMA_Abort
  - >> HAL_UARTEx_RxEventCallback
  - >> UART_Receive_IT
  - >> UART_EndRxTransfer
  - >> HAL_UART_TxCpltCallback
  - >> HAL_UART_ErrorCallback
  [Called By]
  - >> USART2_IRQHandler

  HAL_UART_Init (Thumb, 100 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Init))
  [Stack]

  - Max Depth = 96
  - Call Chain = HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_MspInit
  - >> UART_SetConfig
  [Called By]
  - >> MX_USART2_UART_Init

  HAL_UART_MspInit (Thumb, 254 bytes, Stack size 40 bytes, usart.o(i.HAL_UART_MspInit))
  [Stack]

  - Max Depth = 80
  - Call Chain = HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_DMA_Init
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_Init
  - >> Error_Handler
  [Called By]
  - >> HAL_UART_Init
  - >> HAL_HalfDuplex_Init

  HAL_UART_Receive_DMA (Thumb, 28 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Receive_DMA))
  [Stack]

  - Max Depth = 44
  - Call Chain = HAL_UART_Receive_DMA ⇒ UART_Start_Receive_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> UART_Start_Receive_DMA
  [Called By]
  - >> USAR_UART_IDLECallback

  HAL_UART_RxCpltCallback (Thumb, 34 bytes, Stack size 8 bytes, uart.o(i.HAL_UART_RxCpltCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UART_RxCpltCallback
  [Calls]
  - >> UART_Get
  [Called By]
  - >> UART_Receive_IT
  - >> UART_DMAReceiveCplt

  HAL_UART_RxHalfCpltCallback (Thumb, 34 bytes, Stack size 8 bytes, uart.o(i.HAL_UART_RxHalfCpltCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UART_RxHalfCpltCallback
  [Calls]
  - >> UART_Get
  [Called By]
  - >> UART_DMARxHalfCplt

  HAL_UART_Transmit (Thumb, 160 bytes, Stack size 32 bytes, stm32f1xx_hal_uart.o(i.HAL_UART_Transmit))
  [Stack]

  - Max Depth = 64
  - Call Chain = HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_WaitOnFlagUntilTimeout
  [Called By]
  - >> USAR_UART_IDLECallback
  - >> fputc

  HAL_UART_TxCpltCallback (Thumb, 34 bytes, Stack size 8 bytes, uart.o(i.HAL_UART_TxCpltCallback))
  [Stack]

  - Max Depth = 8
  - Call Chain = HAL_UART_TxCpltCallback
  [Calls]
  - >> UART_Get
  [Called By]
  - >> HAL_UART_IRQHandler

  HardFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.HardFault_Handler))
  [Calls]

  - >> HardFault_Handler
  [Called By]
  - >> HardFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  LCD_Clear (Thumb, 82 bytes, Stack size 24 bytes, lcd.o(i.LCD_Clear))
  [Stack]

  - Max Depth = 208
  - Call Chain = LCD_Clear ⇒ LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> LCD_WriteDataBuffer_DMA
  - >> LCD_SetAddressWindow
  - >> malloc
  - >> free
  [Called By]
  - >> main

  LCD_DrawBitmap (Thumb, 128 bytes, Stack size 56 bytes, lcd.o(i.LCD_DrawBitmap))
  [Stack]

  - Max Depth = 256
  - Call Chain = LCD_DrawBitmap ⇒ LCD_DrawPoint ⇒ LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> main

  LCD_DrawChar (Thumb, 342 bytes, Stack size 64 bytes, lcd.o(i.LCD_DrawChar))
  [Stack]

  - Max Depth = 264
  - Call Chain = LCD_DrawChar ⇒ LCD_DrawPoint ⇒ LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> LCD_DrawPoint
  [Called By]
  - >> LCD_DrawString

  LCD_DrawPoint (Thumb, 88 bytes, Stack size 16 bytes, lcd.o(i.LCD_DrawPoint))
  [Stack]

  - Max Depth = 200
  - Call Chain = LCD_DrawPoint ⇒ LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> LCD_WriteDataBuffer
  - >> LCD_SetAddressWindow
  [Called By]
  - >> LCD_DrawBitmap
  - >> LCD_DrawChar

  LCD_DrawString (Thumb, 110 bytes, Stack size 64 bytes, lcd.o(i.LCD_DrawString))
  [Stack]

  - Max Depth = 328
  - Call Chain = LCD_DrawString ⇒ LCD_DrawChar ⇒ LCD_DrawPoint ⇒ LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> LCD_DrawChar
  [Called By]
  - >> main

  LCD_Init (Thumb, 304 bytes, Stack size 56 bytes, lcd.o(i.LCD_Init))
  [Stack]

  - Max Depth = 208
  - Call Chain = LCD_Init ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> HAL_Delay
  - >> LCD_WriteDataBuffer
  - >> LCD_WriteData
  - >> LCD_WriteCommand
  [Called By]
  - >> main

  MSP_GetIRQn (Thumb, 58 bytes, Stack size 4 bytes, sx1281_driver_gpio.o(i.MSP_GetIRQn))
  [Stack]

  - Max Depth = 4
  - Call Chain = MSP_GetIRQn
  [Calls]
  - >> GpioGetBitPos
  [Called By]
  - >> GpioSetIrq

  MX_DMA_Init (Thumb, 104 bytes, Stack size 8 bytes, dma.o(i.MX_DMA_Init))
  [Stack]

  - Max Depth = 24
  - Call Chain = MX_DMA_Init ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  [Called By]
  - >> main

  MX_GPIO_Init (Thumb, 258 bytes, Stack size 48 bytes, gpio.o(i.MX_GPIO_Init))
  [Stack]

  - Max Depth = 88
  - Call Chain = MX_GPIO_Init ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_NVIC_SetPriority
  - >> HAL_NVIC_EnableIRQ
  - >> HAL_GPIO_WritePin
  - >> HAL_GPIO_Init
  [Called By]
  - >> main

  MX_SPI1_Init (Thumb, 62 bytes, Stack size 8 bytes, spi.o(i.MX_SPI1_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_SPI1_Init ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_SPI2_Init (Thumb, 62 bytes, Stack size 8 bytes, spi.o(i.MX_SPI2_Init))
  [Stack]

  - Max Depth = 112
  - Call Chain = MX_SPI2_Init ⇒ HAL_SPI_Init ⇒ HAL_SPI_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_SPI_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_TIM1_Init (Thumb, 188 bytes, Stack size 96 bytes, tim.o(i.MX_TIM1_Init))
  [Stack]

  - Max Depth = 160
  - Call Chain = MX_TIM1_Init ⇒ HAL_TIM_MspPostInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_PWM_ConfigChannel
  - >> HAL_TIM_ConfigClockSource
  - >> HAL_TIM_Base_Init
  - >> HAL_TIMEx_MasterConfigSynchronization
  - >> HAL_TIMEx_ConfigBreakDeadTime
  - >> HAL_TIM_MspPostInit
  - >> Error_Handler
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  MX_USART1_UART_Init (Thumb, 48 bytes, Stack size 8 bytes, usart.o(i.MX_USART1_UART_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = MX_USART1_UART_Init ⇒ HAL_HalfDuplex_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_HalfDuplex_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MX_USART2_UART_Init (Thumb, 48 bytes, Stack size 8 bytes, usart.o(i.MX_USART2_UART_Init))
  [Stack]

  - Max Depth = 104
  - Call Chain = MX_USART2_UART_Init ⇒ HAL_UART_Init ⇒ HAL_UART_MspInit ⇒ HAL_GPIO_Init
  [Calls]
  - >> HAL_UART_Init
  - >> Error_Handler
  [Called By]
  - >> main

  MemManage_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.MemManage_Handler))
  [Calls]

  - >> MemManage_Handler
  [Called By]
  - >> MemManage_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  NMI_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.NMI_Handler))
  [Calls]

  - >> NMI_Handler
  [Called By]
  - >> NMI_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  OnRxDone (Thumb, 14 bytes, Stack size 8 bytes, sx1281.o(i.OnRxDone))
  [Stack]

  - Max Depth = 56
  - Call Chain = OnRxDone ⇒ SX1281_Callback ⇒ __2printf
  [Calls]
  - >> SX1281_Callback
  [Address Reference Count : 1]
  - sx1281.o(.data)

  OnRxError (Thumb, 14 bytes, Stack size 8 bytes, sx1281.o(i.OnRxError))
  [Stack]

  - Max Depth = 56
  - Call Chain = OnRxError ⇒ SX1281_Callback ⇒ __2printf
  [Calls]
  - >> SX1281_Callback
  [Address Reference Count : 1]
  - sx1281.o(.data)

  OnRxTimeout (Thumb, 14 bytes, Stack size 8 bytes, sx1281.o(i.OnRxTimeout))
  [Stack]

  - Max Depth = 56
  - Call Chain = OnRxTimeout ⇒ SX1281_Callback ⇒ __2printf
  [Calls]
  - >> SX1281_Callback
  [Address Reference Count : 1]
  - sx1281.o(.data)

  OnTxDone (Thumb, 14 bytes, Stack size 8 bytes, sx1281.o(i.OnTxDone))
  [Stack]

  - Max Depth = 56
  - Call Chain = OnTxDone ⇒ SX1281_Callback ⇒ __2printf
  [Calls]
  - >> SX1281_Callback
  [Address Reference Count : 1]
  - sx1281.o(.data)

  OnTxTimeout (Thumb, 14 bytes, Stack size 8 bytes, sx1281.o(i.OnTxTimeout))
  [Stack]

  - Max Depth = 56
  - Call Chain = OnTxTimeout ⇒ SX1281_Callback ⇒ __2printf
  [Calls]
  - >> SX1281_Callback
  [Address Reference Count : 1]
  - sx1281.o(.data)

  PendSV_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.PendSV_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SVC_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SVC_Handler))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(RESET)

  SX1281Calibrate (Thumb, 62 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281Calibrate))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281Calibrate ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281ClearIrqStatus (Thumb, 24 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281ClearIrqStatus))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281ClearIrqStatus ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Called By]
  - >> SX1281SetTx
  - >> SX1281SetRx
  - >> SX1281ProcessIrqs
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetFirmwareVersion (Thumb, 26 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281GetFirmwareVersion))
  [Stack]

  - Max Depth = 184
  - Call Chain = SX1281GetFirmwareVersion ⇒ SX1281HalReadRegister ⇒ SX1281HalReadRegisters ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadRegister
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetFrequencyError (Thumb, 132 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281GetFrequencyError))
  [Stack]

  - Max Depth = 192
  - Call Chain = SX1281GetFrequencyError ⇒ SX1281HalReadRegister ⇒ SX1281HalReadRegisters ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> __aeabi_i2d
  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> SX1281HalReadRegister
  - >> SX1281GetLoRaBandwidth
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetIrqStatus (Thumb, 20 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281GetIrqStatus))
  [Stack]

  - Max Depth = 176
  - Call Chain = SX1281GetIrqStatus ⇒ SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadCommand
  [Called By]
  - >> SX1281ProcessIrqs
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetLoRaBandwidth (Thumb, 38 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281GetLoRaBandwidth))
  [Called By]

  - >> SX1281GetFrequencyError

  SX1281GetOpMode (Thumb, 6 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281GetOpMode))
  [Address Reference Count : 1]

  - sx1281_driver_hal.o(.constdata)

  SX1281GetPacketStatus (Thumb, 526 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281GetPacketStatus))
  [Stack]

  - Max Depth = 184
  - Call Chain = SX1281GetPacketStatus ⇒ SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetPacketType (Thumb, 6 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281GetPacketType))
  [Address Reference Count : 1]

  - sx1281_driver_hal.o(.constdata)

  SX1281GetPayload (Thumb, 40 bytes, Stack size 24 bytes, sx1281_driver.o(i.SX1281GetPayload))
  [Stack]

  - Max Depth = 224
  - Call Chain = SX1281GetPayload ⇒ SX1281GetRxBufferStatus ⇒ SX1281HalReadRegister ⇒ SX1281HalReadRegisters ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadBuffer
  - >> SX1281GetRxBufferStatus
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetRssiInst (Thumb, 34 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281GetRssiInst))
  [Stack]

  - Max Depth = 176
  - Call Chain = SX1281GetRssiInst ⇒ SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetRxBufferStatus (Thumb, 68 bytes, Stack size 24 bytes, sx1281_driver.o(i.SX1281GetRxBufferStatus))
  [Stack]

  - Max Depth = 200
  - Call Chain = SX1281GetRxBufferStatus ⇒ SX1281HalReadRegister ⇒ SX1281HalReadRegisters ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadRegister
  - >> SX1281HalReadCommand
  [Called By]
  - >> SX1281GetPayload
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281GetStatus (Thumb, 24 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281GetStatus))
  [Stack]

  - Max Depth = 176
  - Call Chain = SX1281GetStatus ⇒ SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalGetDioStatus (Thumb, 32 bytes, Stack size 16 bytes, sx1281_driver_hal.o(i.SX1281HalGetDioStatus))
  [Stack]

  - Max Depth = 16
  - Call Chain = SX1281HalGetDioStatus
  [Calls]
  - >> GpioRead
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalInit (Thumb, 18 bytes, Stack size 8 bytes, sx1281_driver_hal.o(i.SX1281HalInit))
  [Stack]

  - Max Depth = 40
  - Call Chain = SX1281HalInit ⇒ SX1281HalIoIrqInit ⇒ GpioSetIrq ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> SX1281HalReset
  - >> SX1281HalIoIrqInit
  [Called By]
  - >> SX1281Init

  SX1281HalIoIrqInit (Thumb, 12 bytes, Stack size 0 bytes, sx1281_driver_hal.o(i.SX1281HalIoIrqInit))
  [Stack]

  - Max Depth = 32
  - Call Chain = SX1281HalIoIrqInit ⇒ GpioSetIrq ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> GpioSetIrq
  [Called By]
  - >> SX1281HalInit

  SX1281HalReadBuffer (Thumb, 96 bytes, Stack size 24 bytes, sx1281_driver_hal.o(i.SX1281HalReadBuffer))
  [Stack]

  - Max Depth = 168
  - Call Chain = SX1281HalReadBuffer ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SpiInOut
  - >> SX1281HalWaitOnBusy
  - >> GpioWrite
  - >> __aeabi_memcpy
  [Called By]
  - >> SX1281GetPayload
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalReadCommand (Thumb, 94 bytes, Stack size 24 bytes, sx1281_driver_hal.o(i.SX1281HalReadCommand))
  [Stack]

  - Max Depth = 168
  - Call Chain = SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SpiInOut
  - >> SX1281HalWaitOnBusy
  - >> GpioWrite
  - >> __aeabi_memcpy
  [Called By]
  - >> SX1281GetStatus
  - >> SX1281GetRxBufferStatus
  - >> SX1281GetRssiInst
  - >> SX1281GetPacketStatus
  - >> SX1281GetIrqStatus
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalReadRegister (Thumb, 16 bytes, Stack size 8 bytes, sx1281_driver_hal.o(i.SX1281HalReadRegister))
  [Stack]

  - Max Depth = 176
  - Call Chain = SX1281HalReadRegister ⇒ SX1281HalReadRegisters ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalReadRegisters
  [Called By]
  - >> SX1281SetSyncWordErrorTolerance
  - >> SX1281GetRxBufferStatus
  - >> SX1281GetFrequencyError
  - >> SX1281GetFirmwareVersion
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalReadRegisters (Thumb, 100 bytes, Stack size 24 bytes, sx1281_driver_hal.o(i.SX1281HalReadRegisters))
  [Stack]

  - Max Depth = 168
  - Call Chain = SX1281HalReadRegisters ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SpiInOut
  - >> SX1281HalWaitOnBusy
  - >> GpioWrite
  - >> __aeabi_memcpy
  [Called By]
  - >> SX1281HalReadRegister
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalReset (Thumb, 46 bytes, Stack size 8 bytes, sx1281_driver_hal.o(i.SX1281HalReset))
  [Stack]

  - Max Depth = 24
  - Call Chain = SX1281HalReset ⇒ HAL_Delay
  [Calls]
  - >> HAL_Delay
  - >> GpioWrite
  [Called By]
  - >> SX1281HalInit
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalWaitOnBusy (Thumb, 22 bytes, Stack size 16 bytes, sx1281_driver_hal.o(i.SX1281HalWaitOnBusy))
  [Stack]

  - Max Depth = 16
  - Call Chain = SX1281HalWaitOnBusy
  [Calls]
  - >> HAL_GPIO_ReadPin
  [Called By]
  - >> SX1281HalReadRegisters
  - >> SX1281HalWriteRegisters
  - >> SX1281HalWriteCommand
  - >> SX1281HalWriteBuffer
  - >> SX1281HalReadCommand
  - >> SX1281HalReadBuffer

  SX1281HalWriteBuffer (Thumb, 64 bytes, Stack size 16 bytes, sx1281_driver_hal.o(i.SX1281HalWriteBuffer))
  [Stack]

  - Max Depth = 120
  - Call Chain = SX1281HalWriteBuffer ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SpiIn
  - >> SX1281HalWaitOnBusy
  - >> GpioWrite
  - >> __aeabi_memcpy
  [Called By]
  - >> SX1281SetPayload
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalWriteCommand (Thumb, 78 bytes, Stack size 24 bytes, sx1281_driver_hal.o(i.SX1281HalWriteCommand))
  [Stack]

  - Max Depth = 128
  - Call Chain = SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SpiIn
  - >> SX1281HalWaitOnBusy
  - >> GpioWrite
  - >> __aeabi_memcpy
  [Called By]
  - >> SX1281SetTxParams
  - >> SX1281SetTxContinuousWave
  - >> SX1281SetTxContinuousPreamble
  - >> SX1281SetTx
  - >> SX1281SetStandby
  - >> SX1281SetSleep
  - >> SX1281SetSaveContext
  - >> SX1281SetRxDutyCycle
  - >> SX1281SetRx
  - >> SX1281SetRfFrequency
  - >> SX1281SetRegulatorMode
  - >> SX1281SetPacketType
  - >> SX1281SetPacketParams
  - >> SX1281SetModulationParams
  - >> SX1281SetLongPreamble
  - >> SX1281SetFs
  - >> SX1281SetDioIrqParams
  - >> SX1281SetCadParams
  - >> SX1281SetCad
  - >> SX1281SetBufferBaseAddresses
  - >> SX1281SetAutoTx
  - >> SX1281SetAutoFS
  - >> SX1281ClearIrqStatus
  - >> SX1281Calibrate
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalWriteRegister (Thumb, 12 bytes, Stack size 16 bytes, sx1281_driver_hal.o(i.SX1281HalWriteRegister))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281HalWriteRegister ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegisters
  [Called By]
  - >> SX1281SetWhiteningSeed
  - >> SX1281SetSyncWordErrorTolerance
  - >> SX1281SetRegistersDefault
  - >> SX1281SetBleAccessAddress
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281HalWriteRegisters (Thumb, 72 bytes, Stack size 16 bytes, sx1281_driver_hal.o(i.SX1281HalWriteRegisters))
  [Stack]

  - Max Depth = 120
  - Call Chain = SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SpiIn
  - >> SX1281HalWaitOnBusy
  - >> GpioWrite
  - >> __aeabi_memcpy
  [Called By]
  - >> SX1281HalWriteRegister
  - >> SX1281SetSyncWord
  - >> SX1281SetCrcSeed
  - >> SX1281SetCrcPolynomial
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281Init (Thumb, 12 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281Init))
  [Stack]

  - Max Depth = 40
  - Call Chain = SX1281Init ⇒ SX1281HalInit ⇒ SX1281HalIoIrqInit ⇒ GpioSetIrq ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> SX1281HalInit
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281OnDioIrq (Thumb, 16 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281OnDioIrq))
  [Stack]

  - Max Depth = 192
  - Call Chain = SX1281OnDioIrq ⇒ SX1281ProcessIrqs ⇒ SX1281GetIrqStatus ⇒ SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281ProcessIrqs
  [Address Reference Count : 1]
  - sx1281_driver.o(.data)

  SX1281ProcessIrqs (Thumb, 328 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281ProcessIrqs))
  [Stack]

  - Max Depth = 192
  - Call Chain = SX1281ProcessIrqs ⇒ SX1281GetIrqStatus ⇒ SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281GetIrqStatus
  - >> SX1281ClearIrqStatus
  [Called By]
  - >> SX1281_Running
  - >> SX1281OnDioIrq

  SX1281SendPayload (Thumb, 18 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SendPayload))
  [Stack]

  - Max Depth = 152
  - Call Chain = SX1281SendPayload ⇒ SX1281SetTx ⇒ SX1281ClearIrqStatus ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281SetTx
  - >> SX1281SetPayload
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetAutoFS (Thumb, 14 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetAutoFS))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetAutoFS ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetAutoTx (Thumb, 26 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetAutoTx))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetAutoTx ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetBleAccessAddress (Thumb, 52 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetBleAccessAddress))
  [Stack]

  - Max Depth = 144
  - Call Chain = SX1281SetBleAccessAddress ⇒ SX1281HalWriteRegister ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegister
  [Called By]
  - >> SX1281SetBleAdvertizerAccessAddress
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetBleAdvertizerAccessAddress (Thumb, 6 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetBleAdvertizerAccessAddress))
  [Stack]

  - Max Depth = 144
  - Call Chain = SX1281SetBleAdvertizerAccessAddress ⇒ SX1281SetBleAccessAddress ⇒ SX1281HalWriteRegister ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281SetBleAccessAddress
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetBufferBaseAddresses (Thumb, 22 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetBufferBaseAddresses))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetBufferBaseAddresses ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetCad (Thumb, 20 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetCad))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetCad ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetCadParams (Thumb, 20 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetCadParams))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetCadParams ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetCrcPolynomial (Thumb, 36 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetCrcPolynomial))
  [Stack]

  - Max Depth = 128
  - Call Chain = SX1281SetCrcPolynomial ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegisters
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetCrcSeed (Thumb, 36 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetCrcSeed))
  [Stack]

  - Max Depth = 128
  - Call Chain = SX1281SetCrcSeed ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegisters
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetDioIrqParams (Thumb, 54 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281SetDioIrqParams))
  [Stack]

  - Max Depth = 144
  - Call Chain = SX1281SetDioIrqParams ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetFs (Thumb, 20 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetFs))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetFs ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetInterruptMode (Thumb, 8 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetInterruptMode))
  [Address Reference Count : 1]

  - sx1281_driver_hal.o(.constdata)

  SX1281SetLongPreamble (Thumb, 14 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetLongPreamble))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetLongPreamble ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetModulationParams (Thumb, 142 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281SetModulationParams))
  [Stack]

  - Max Depth = 152
  - Call Chain = SX1281SetModulationParams ⇒ SX1281SetPacketType ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  - >> SX1281SetPacketType
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetPacketParams (Thumb, 212 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281SetPacketParams))
  [Stack]

  - Max Depth = 152
  - Call Chain = SX1281SetPacketParams ⇒ SX1281SetPacketType ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  - >> SX1281SetPacketType
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetPacketType (Thumb, 22 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetPacketType))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetPacketType ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Called By]
  - >> SX1281SetPacketParams
  - >> SX1281SetModulationParams
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetPayload (Thumb, 10 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetPayload))
  [Stack]

  - Max Depth = 120
  - Call Chain = SX1281SetPayload ⇒ SX1281HalWriteBuffer ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteBuffer
  [Called By]
  - >> SX1281SendPayload
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetPollingMode (Thumb, 8 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetPollingMode))
  [Address Reference Count : 1]

  - sx1281_driver_hal.o(.constdata)

  SX1281SetRegistersDefault (Thumb, 32 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281SetRegistersDefault))
  [Stack]

  - Max Depth = 152
  - Call Chain = SX1281SetRegistersDefault ⇒ SX1281HalWriteRegister ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegister
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetRegulatorMode (Thumb, 14 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetRegulatorMode))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetRegulatorMode ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetRfFrequency (Thumb, 46 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetRfFrequency))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetRfFrequency ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> __aeabi_ui2d
  - >> __aeabi_ddiv
  - >> __aeabi_d2uiz
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetRx (Thumb, 44 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetRx))
  [Stack]

  - Max Depth = 144
  - Call Chain = SX1281SetRx ⇒ SX1281ClearIrqStatus ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  - >> SX1281ClearIrqStatus
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetRxDutyCycle (Thumb, 44 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281SetRxDutyCycle))
  [Stack]

  - Max Depth = 144
  - Call Chain = SX1281SetRxDutyCycle ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetSaveContext (Thumb, 10 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetSaveContext))
  [Stack]

  - Max Depth = 128
  - Call Chain = SX1281SetSaveContext ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetSleep (Thumb, 50 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetSleep))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetSleep ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetStandby (Thumb, 30 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetStandby))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetStandby ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetSyncWord (Thumb, 104 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetSyncWord))
  [Stack]

  - Max Depth = 128
  - Call Chain = SX1281SetSyncWord ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegisters
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetSyncWordErrorTolerance (Thumb, 34 bytes, Stack size 16 bytes, sx1281_driver.o(i.SX1281SetSyncWordErrorTolerance))
  [Stack]

  - Max Depth = 192
  - Call Chain = SX1281SetSyncWordErrorTolerance ⇒ SX1281HalReadRegister ⇒ SX1281HalReadRegisters ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegister
  - >> SX1281HalReadRegister
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetTx (Thumb, 44 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetTx))
  [Stack]

  - Max Depth = 144
  - Call Chain = SX1281SetTx ⇒ SX1281ClearIrqStatus ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  - >> SX1281ClearIrqStatus
  [Called By]
  - >> SX1281SendPayload
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetTxContinuousPreamble (Thumb, 10 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetTxContinuousPreamble))
  [Stack]

  - Max Depth = 128
  - Call Chain = SX1281SetTxContinuousPreamble ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetTxContinuousWave (Thumb, 10 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetTxContinuousWave))
  [Stack]

  - Max Depth = 128
  - Call Chain = SX1281SetTxContinuousWave ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetTxParams (Thumb, 24 bytes, Stack size 8 bytes, sx1281_driver.o(i.SX1281SetTxParams))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetTxParams ⇒ SX1281HalWriteCommand ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteCommand
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281SetWhiteningSeed (Thumb, 26 bytes, Stack size 0 bytes, sx1281_driver.o(i.SX1281SetWhiteningSeed))
  [Stack]

  - Max Depth = 136
  - Call Chain = SX1281SetWhiteningSeed ⇒ SX1281HalWriteRegister ⇒ SX1281HalWriteRegisters ⇒ SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281HalWriteRegister
  [Address Reference Count : 1]
  - sx1281_driver_hal.o(.constdata)

  SX1281_BSPInit (Thumb, 14 bytes, Stack size 8 bytes, sx1281_header.o(i.SX1281_BSPInit))
  [Stack]

  - Max Depth = 16
  - Call Chain = SX1281_BSPInit ⇒ SpiInit
  [Calls]
  - >> SpiInit
  - >> GpioInit
  [Called By]
  - >> SX1281_Init

  SX1281_Callback (Thumb, 126 bytes, Stack size 24 bytes, sx1281.o(i.SX1281_Callback))
  [Stack]

  - Max Depth = 48
  - Call Chain = SX1281_Callback ⇒ __2printf
  [Calls]
  - >> __2printf
  [Called By]
  - >> OnTxTimeout
  - >> OnTxDone
  - >> OnRxTimeout
  - >> OnRxError
  - >> OnRxDone

  SX1281_GetState (Thumb, 20 bytes, Stack size 0 bytes, sx1281.o(i.SX1281_GetState))
  [Called By]

  - >> SX1281_Running

  SX1281_Init (Thumb, 492 bytes, Stack size 48 bytes, sx1281.o(i.SX1281_Init))
  [Stack]

  - Max Depth = 72
  - Call Chain = SX1281_Init ⇒ __2printf
  [Calls]
  - >> HAL_Delay
  - >> SX1281_BSPInit
  - >> __2printf
  [Called By]
  - >> main

  SX1281_Running (Thumb, 24 bytes, Stack size 8 bytes, sx1281.o(i.SX1281_Running))
  [Stack]

  - Max Depth = 200
  - Call Chain = SX1281_Running ⇒ SX1281ProcessIrqs ⇒ SX1281GetIrqStatus ⇒ SX1281HalReadCommand ⇒ SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_Delay
  - >> SX1281ProcessIrqs
  - >> SX1281_GetState
  [Called By]
  - >> main

  SX1281_SetTX (Thumb, 36 bytes, Stack size 16 bytes, sx1281.o(i.SX1281_SetTX))
  [Stack]

  - Max Depth = 16
  - Call Chain = SX1281_SetTX
  [Called By]
  - >> main

  SpiIn (Thumb, 18 bytes, Stack size 0 bytes, sx1281_driver_spi.o(i.SpiIn))
  [Stack]

  - Max Depth = 104
  - Call Chain = SpiIn ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> BSP_SPI_Transmit
  [Called By]
  - >> SX1281HalWriteRegisters
  - >> SX1281HalWriteCommand
  - >> SX1281HalWriteBuffer

  SpiInOut (Thumb, 26 bytes, Stack size 16 bytes, sx1281_driver_spi.o(i.SpiInOut))
  [Stack]

  - Max Depth = 144
  - Call Chain = SpiInOut ⇒ BSP_SPI_TransmitReceive ⇒ HAL_SPI_TransmitReceive ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> BSP_SPI_TransmitReceive
  [Called By]
  - >> SX1281HalReadRegisters
  - >> SX1281HalReadCommand
  - >> SX1281HalReadBuffer

  SpiInit (Thumb, 26 bytes, Stack size 8 bytes, sx1281_driver_spi.o(i.SpiInit))
  [Stack]

  - Max Depth = 8
  - Call Chain = SpiInit
  [Calls]
  - >> BSP_SPI_RegisterCallback
  [Called By]
  - >> SX1281_BSPInit

  SysTick_Handler (Thumb, 4 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.SysTick_Handler))
  [Calls]

  - >> HAL_IncTick
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  SystemClock_Config (Thumb, 96 bytes, Stack size 72 bytes, main.o(i.SystemClock_Config))
  [Stack]

  - Max Depth = 136
  - Call Chain = SystemClock_Config ⇒ HAL_RCC_ClockConfig ⇒ HAL_InitTick ⇒ HAL_NVIC_SetPriority
  [Calls]
  - >> HAL_RCC_OscConfig
  - >> HAL_RCC_ClockConfig
  - >> __aeabi_memclr4
  [Called By]
  - >> main

  SystemInit (Thumb, 2 bytes, Stack size 0 bytes, system_stm32f1xx.o(i.SystemInit))
  [Address Reference Count : 1]

  - startup_stm32f103xb.o(.text)

  TIM_Base_SetConfig (Thumb, 108 bytes, Stack size 20 bytes, stm32f1xx_hal_tim.o(i.TIM_Base_SetConfig))
  [Stack]

  - Max Depth = 20
  - Call Chain = TIM_Base_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_Init
  - >> HAL_TIM_Base_Init

  TIM_ETR_SetConfig (Thumb, 20 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_ETR_SetConfig))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_ETR_SetConfig
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_OC2_SetConfig (Thumb, 84 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC2_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC2_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  UART_Start_Receive_DMA (Thumb, 130 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA))
  [Stack]

  - Max Depth = 44
  - Call Chain = UART_Start_Receive_DMA ⇒ HAL_DMA_Start_IT ⇒ DMA_SetConfig
  [Calls]
  - >> HAL_DMA_Start_IT
  [Called By]
  - >> HAL_UART_Receive_DMA

  USART2_IRQHandler (Thumb, 18 bytes, Stack size 8 bytes, stm32f1xx_it.o(i.USART2_IRQHandler))
  [Stack]

  - Max Depth = 104
  - Call Chain = USART2_IRQHandler ⇒ USER_UART_IRQHandler ⇒ USAR_UART_IDLECallback ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_IRQHandler
  - >> USER_UART_IRQHandler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  USAR_UART_IDLECallback (Thumb, 102 bytes, Stack size 16 bytes, usart.o(i.USAR_UART_IDLECallback))
  [Stack]

  - Max Depth = 80
  - Call Chain = USAR_UART_IDLECallback ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> HAL_UART_Receive_DMA
  - >> HAL_UART_DMAStop
  - >> strcpy
  - >> __aeabi_memclr4
  - >> __2printf
  [Called By]
  - >> USER_UART_IRQHandler

  USER_UART_IRQHandler (Thumb, 46 bytes, Stack size 16 bytes, usart.o(i.USER_UART_IRQHandler))
  [Stack]

  - Max Depth = 96
  - Call Chain = USER_UART_IRQHandler ⇒ USAR_UART_IDLECallback ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> USAR_UART_IDLECallback
  - >> __2printf
  [Called By]
  - >> USART2_IRQHandler

  UsageFault_Handler (Thumb, 2 bytes, Stack size 0 bytes, stm32f1xx_it.o(i.UsageFault_Handler))
  [Calls]

  - >> UsageFault_Handler
  [Called By]
  - >> UsageFault_Handler
  [Address Reference Count : 1]
  - startup_stm32f103xb.o(RESET)

  __0printf (Thumb, 22 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)
  [Calls]

  - >> _printf_core

  __1printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __2printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf))
  [Stack]

  - Max Depth = 24
  - Call Chain = __2printf
  [Called By]
  - >> USER_UART_IRQHandler
  - >> USAR_UART_IDLECallback
  - >> SX1281_Init
  - >> SX1281_Callback

  __c89printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  printf (Thumb, 0 bytes, Stack size 24 bytes, printfa.o(i.__0printf), UNUSED)

  __scatterload_copy (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_copy), UNUSED)

  __scatterload_null (Thumb, 2 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_null), UNUSED)

  __scatterload_zeroinit (Thumb, 14 bytes, Stack size unknown bytes, handlers.o(i.__scatterload_zeroinit), UNUSED)

  fputc (Thumb, 24 bytes, Stack size 16 bytes, sx1281_header.o(i.fputc))
  [Stack]

  - Max Depth = 80
  - Call Chain = fputc ⇒ HAL_UART_Transmit ⇒ UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_UART_Transmit
  - >> BSP_UART_GetHandle
  [Address Reference Count : 1]
  - printfa.o(i.__0printf)

  free (Thumb, 76 bytes, Stack size 8 bytes, malloc.o(i.free))
  [Stack]

  - Max Depth = 8
  - Call Chain = free
  [Called By]
  - >> LCD_Clear

  main (Thumb, 134 bytes, Stack size 16 bytes, main.o(i.main))
  [Stack]

  - Max Depth = 344
  - Call Chain = main ⇒ LCD_DrawString ⇒ LCD_DrawChar ⇒ LCD_DrawPoint ⇒ LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SX1281_SetTX
  - >> SX1281_Running
  - >> SX1281_Init
  - >> MX_USART2_UART_Init
  - >> MX_USART1_UART_Init
  - >> MX_TIM1_Init
  - >> MX_SPI2_Init
  - >> MX_SPI1_Init
  - >> MX_GPIO_Init
  - >> MX_DMA_Init
  - >> LCD_Init
  - >> LCD_DrawString
  - >> LCD_DrawBitmap
  - >> LCD_Clear
  - >> HAL_Init
  - >> HAL_Delay
  - >> SystemClock_Config
  [Address Reference Count : 1]
  - entry9a.o(.ARM.Collect$$$$0000000B)

  malloc (Thumb, 92 bytes, Stack size 20 bytes, malloc.o(i.malloc))
  [Stack]

  - Max Depth = 20
  - Call Chain = malloc
  [Called By]
  - >> LCD_Clear

  ### Local Symbols

  SPI_DMAError (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.SPI_DMAError))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_DMAError ⇒ HAL_SPI_ErrorCallback
  [Calls]
  - >> HAL_SPI_ErrorCallback
  [Address Reference Count : 2]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)
  - stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)

  SPI_DMAHalfReceiveCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.SPI_DMAHalfReceiveCplt))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_DMAHalfReceiveCplt ⇒ HAL_SPI_RxHalfCpltCallback
  [Calls]
  - >> HAL_SPI_RxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)

  SPI_DMAHalfTransmitCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitCplt))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_DMAHalfTransmitCplt ⇒ HAL_SPI_TxHalfCpltCallback
  [Calls]
  - >> HAL_SPI_TxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)

  SPI_DMAHalfTransmitReceiveCplt (Thumb, 10 bytes, Stack size 8 bytes, stm32f1xx_hal_spi.o(i.SPI_DMAHalfTransmitReceiveCplt))
  [Stack]

  - Max Depth = 24
  - Call Chain = SPI_DMAHalfTransmitReceiveCplt ⇒ HAL_SPI_TxRxHalfCpltCallback
  [Calls]
  - >> HAL_SPI_TxRxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)

  SPI_DMAReceiveCplt (Thumb, 106 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.SPI_DMAReceiveCplt))
  [Stack]

  - Max Depth = 72
  - Call Chain = SPI_DMAReceiveCplt ⇒ SPI_EndRxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_EndRxTransaction
  - >> HAL_GetTick
  - >> HAL_SPI_RxCpltCallback
  - >> HAL_SPI_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)

  SPI_DMATransmitCplt (Thumb, 100 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.SPI_DMATransmitCplt))
  [Stack]

  - Max Depth = 72
  - Call Chain = SPI_DMATransmitCplt ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_EndRxTxTransaction
  - >> HAL_GetTick
  - >> HAL_SPI_TxCpltCallback
  - >> HAL_SPI_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_Transmit_DMA)

  SPI_DMATransmitReceiveCplt (Thumb, 90 bytes, Stack size 16 bytes, stm32f1xx_hal_spi.o(i.SPI_DMATransmitReceiveCplt))
  [Stack]

  - Max Depth = 72
  - Call Chain = SPI_DMATransmitReceiveCplt ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_EndRxTxTransaction
  - >> HAL_GetTick
  - >> HAL_SPI_TxRxCpltCallback
  - >> HAL_SPI_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_spi.o(i.HAL_SPI_TransmitReceive_DMA)

  SPI_EndRxTransaction (Thumb, 92 bytes, Stack size 24 bytes, stm32f1xx_hal_spi.o(i.SPI_EndRxTransaction))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPI_EndRxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_WaitFlagStateUntilTimeout
  [Called By]
  - >> SPI_DMAReceiveCplt

  SPI_EndRxTxTransaction (Thumb, 52 bytes, Stack size 24 bytes, stm32f1xx_hal_spi.o(i.SPI_EndRxTxTransaction))
  [Stack]

  - Max Depth = 56
  - Call Chain = SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> SPI_WaitFlagStateUntilTimeout
  [Called By]
  - >> SPI_DMATransmitReceiveCplt
  - >> SPI_DMATransmitCplt
  - >> HAL_SPI_TransmitReceive
  - >> HAL_SPI_Transmit

  SPI_WaitFlagStateUntilTimeout (Thumb, 180 bytes, Stack size 32 bytes, stm32f1xx_hal_spi.o(i.SPI_WaitFlagStateUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GetTick
  [Called By]
  - >> SPI_EndRxTxTransaction
  - >> SPI_EndRxTransaction

  DMA_SetConfig (Thumb, 42 bytes, Stack size 12 bytes, stm32f1xx_hal_dma.o(i.DMA_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = DMA_SetConfig
  [Called By]
  - >> HAL_DMA_Start_IT

  __NVIC_SetPriority (Thumb, 32 bytes, Stack size 0 bytes, stm32f1xx_hal_cortex.o(i.__NVIC_SetPriority))
  [Called By]

  - >> HAL_NVIC_SetPriority
  - >> HAL_SYSTICK_Config

  TIM_ITRx_SetConfig (Thumb, 16 bytes, Stack size 0 bytes, stm32f1xx_hal_tim.o(i.TIM_ITRx_SetConfig))
  [Called By]

  - >> HAL_TIM_ConfigClockSource

  TIM_OC1_SetConfig (Thumb, 74 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC1_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC1_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC3_SetConfig (Thumb, 82 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC3_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC3_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_OC4_SetConfig (Thumb, 64 bytes, Stack size 12 bytes, stm32f1xx_hal_tim.o(i.TIM_OC4_SetConfig))
  [Stack]

  - Max Depth = 12
  - Call Chain = TIM_OC4_SetConfig
  [Called By]
  - >> HAL_TIM_PWM_ConfigChannel

  TIM_TI1_ConfigInputStage (Thumb, 34 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI1_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI1_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  TIM_TI2_ConfigInputStage (Thumb, 36 bytes, Stack size 8 bytes, stm32f1xx_hal_tim.o(i.TIM_TI2_ConfigInputStage))
  [Stack]

  - Max Depth = 8
  - Call Chain = TIM_TI2_ConfigInputStage
  [Called By]
  - >> HAL_TIM_ConfigClockSource

  UART_DMAAbortOnError (Thumb, 16 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_DMAAbortOnError))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMAAbortOnError ⇒ HAL_UART_ErrorCallback
  [Calls]
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_uart.o(i.HAL_UART_IRQHandler)

  UART_DMAError (Thumb, 74 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.UART_DMAError))
  [Stack]

  - Max Depth = 24
  - Call Chain = UART_DMAError ⇒ HAL_UART_ErrorCallback
  [Calls]
  - >> UART_EndTxTransfer
  - >> UART_EndRxTransfer
  - >> HAL_UART_ErrorCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA)

  UART_DMAReceiveCplt (Thumb, 134 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_DMAReceiveCplt))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMAReceiveCplt ⇒ HAL_UART_RxCpltCallback
  [Calls]
  - >> HAL_UARTEx_RxEventCallback
  - >> HAL_UART_RxCpltCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA)

  UART_DMARxHalfCplt (Thumb, 30 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_DMARxHalfCplt))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_DMARxHalfCplt ⇒ HAL_UART_RxHalfCpltCallback
  [Calls]
  - >> HAL_UARTEx_RxEventCallback
  - >> HAL_UART_RxHalfCpltCallback
  [Address Reference Count : 1]
  - stm32f1xx_hal_uart.o(i.UART_Start_Receive_DMA)

  UART_EndRxTransfer (Thumb, 78 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_EndRxTransfer))
  [Calls]

  - >> UART_EndRxTransfer
  [Called By]
  - >> HAL_UART_IRQHandler
  - >> HAL_UART_DMAStop
  - >> UART_WaitOnFlagUntilTimeout
  - >> UART_EndRxTransfer
  - >> UART_DMAError

  UART_EndTxTransfer (Thumb, 28 bytes, Stack size 0 bytes, stm32f1xx_hal_uart.o(i.UART_EndTxTransfer))
  [Calls]

  - >> UART_EndTxTransfer
  [Called By]
  - >> HAL_UART_DMAStop
  - >> UART_EndTxTransfer
  - >> UART_DMAError

  UART_Receive_IT (Thumb, 194 bytes, Stack size 8 bytes, stm32f1xx_hal_uart.o(i.UART_Receive_IT))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_Receive_IT ⇒ HAL_UART_RxCpltCallback
  [Calls]
  - >> HAL_UARTEx_RxEventCallback
  - >> HAL_UART_RxCpltCallback
  [Called By]
  - >> HAL_UART_IRQHandler

  UART_SetConfig (Thumb, 178 bytes, Stack size 16 bytes, stm32f1xx_hal_uart.o(i.UART_SetConfig))
  [Stack]

  - Max Depth = 16
  - Call Chain = UART_SetConfig
  [Calls]
  - >> HAL_RCC_GetPCLK2Freq
  - >> HAL_RCC_GetPCLK1Freq
  [Called By]
  - >> HAL_UART_Init
  - >> HAL_HalfDuplex_Init

  UART_WaitOnFlagUntilTimeout (Thumb, 114 bytes, Stack size 32 bytes, stm32f1xx_hal_uart.o(i.UART_WaitOnFlagUntilTimeout))
  [Stack]

  - Max Depth = 32
  - Call Chain = UART_WaitOnFlagUntilTimeout
  [Calls]
  - >> HAL_GetTick
  - >> UART_EndRxTransfer
  [Called By]
  - >> HAL_UART_Transmit

  tx_cplt_cb (Thumb, 8 bytes, Stack size 0 bytes, sx1281_driver_spi.o(i.tx_cplt_cb))
  [Address Reference Count : 1]

  - sx1281_driver_spi.o(i.SpiInit)

  txrx_cplt_cb (Thumb, 8 bytes, Stack size 0 bytes, sx1281_driver_spi.o(i.txrx_cplt_cb))
  [Address Reference Count : 1]

  - sx1281_driver_spi.o(i.SpiInit)

  SPI_Get (Thumb, 26 bytes, Stack size 0 bytes, spi_1.o(i.SPI_Get))
  [Called By]

  - >> HAL_SPI_TxRxHalfCpltCallback
  - >> HAL_SPI_TxRxCpltCallback
  - >> HAL_SPI_TxHalfCpltCallback
  - >> HAL_SPI_TxCpltCallback
  - >> HAL_SPI_RxHalfCpltCallback
  - >> HAL_SPI_RxCpltCallback
  - >> HAL_SPI_ErrorCallback

  UART_Get (Thumb, 16 bytes, Stack size 0 bytes, uart.o(i.UART_Get))
  [Called By]

  - >> HAL_UART_TxCpltCallback
  - >> HAL_UART_RxHalfCpltCallback
  - >> HAL_UART_RxCpltCallback
  - >> HAL_UART_ErrorCallback

  LCD_SetAddressWindow (Thumb, 100 bytes, Stack size 32 bytes, lcd.o(i.LCD_SetAddressWindow))
  [Stack]

  - Max Depth = 184
  - Call Chain = LCD_SetAddressWindow ⇒ LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> LCD_WriteDataBuffer
  - >> LCD_WriteCommand
  [Called By]
  - >> LCD_Clear
  - >> LCD_DrawPoint

  LCD_WriteCommand (Thumb, 56 bytes, Stack size 16 bytes, lcd.o(i.LCD_WriteCommand))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_WriteCommand ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> BSP_SPI_Transmit
  [Called By]
  - >> LCD_Init
  - >> LCD_SetAddressWindow

  LCD_WriteData (Thumb, 54 bytes, Stack size 16 bytes, lcd.o(i.LCD_WriteData))
  [Stack]

  - Max Depth = 120
  - Call Chain = LCD_WriteData ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> BSP_SPI_Transmit
  [Called By]
  - >> LCD_Init

  LCD_WriteDataBuffer (Thumb, 72 bytes, Stack size 24 bytes, lcd.o(i.LCD_WriteDataBuffer))
  [Stack]

  - Max Depth = 152
  - Call Chain = LCD_WriteDataBuffer ⇒ LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> BSP_SPI_Transmit
  - >> LCD_WriteDataBuffer_DMA
  [Called By]
  - >> LCD_Init
  - >> LCD_DrawPoint
  - >> LCD_SetAddressWindow

  LCD_WriteDataBuffer_DMA (Thumb, 72 bytes, Stack size 24 bytes, lcd.o(i.LCD_WriteDataBuffer_DMA))
  [Stack]

  - Max Depth = 128
  - Call Chain = LCD_WriteDataBuffer_DMA ⇒ BSP_SPI_Transmit ⇒ HAL_SPI_Transmit ⇒ SPI_EndRxTxTransaction ⇒ SPI_WaitFlagStateUntilTimeout
  [Calls]
  - >> HAL_GPIO_WritePin
  - >> BSP_SPI_Transmit
  - >> BSP_SPI_GetState
  [Called By]
  - >> LCD_Clear
  - >> LCD_WriteDataBuffer

  _fp_digits (Thumb, 366 bytes, Stack size 64 bytes, printfa.o(i._fp_digits), UNUSED)
  [Calls]

  - >> __aeabi_dmul
  - >> __aeabi_ddiv
  - >> __aeabi_uldivmod
  - >> __aeabi_dadd
  - >> __aeabi_d2ulz
  - >> __aeabi_cdrcmple
  [Called By]
  - >> _printf_core

  _printf_core (Thumb, 1704 bytes, Stack size 136 bytes, printfa.o(i._printf_core), UNUSED)
  [Calls]

  - >> __aeabi_uldivmod
  - >> __aeabi_uidivmod
  - >> _printf_pre_padding
  - >> _printf_post_padding
  - >> _fp_digits
  [Called By]
  - >> __0printf

  _printf_post_padding (Thumb, 36 bytes, Stack size 24 bytes, printfa.o(i._printf_post_padding), UNUSED)
  [Called By]

  - >> _printf_core

  _printf_pre_padding (Thumb, 46 bytes, Stack size 24 bytes, printfa.o(i._printf_pre_padding), UNUSED)
  [Called By]

  - >> _printf_core

  ### Undefined Global Symbols